VertexDSP – MultiInspector
Release Notes

Version 2.3.0 - 24-Mar-2010
Enhancements
	•	Windows x64 version added.

Bug Fixes
	•	Denormal problem fixed.
	•	The AlphaBlend option now also works for the 32bit version in Windows x64.
	•	The measurement cursor now works correctly in V-Space mode.
	•	Fixed a drawing bug under certain circumstances if audio has been bypassed.

Please note that the minimum system requirements are now Windows XP/Mac OS X 10.4. Windows 2000 and Mac OS X 10.3.9 are no longer supported.

Version 2.2.1 - 16-Sep-2008
Enhancements
	•	The GUI can now be resized to show only the frequency display. Click on the 1/3 Oct or on the FFT button in combination with the shift-key to switch to the small GUI.
	•	MultiInspector is now compatible with the fxpansion VST-RTAS adapter for use in ProTools.

Version 2.2.0 - 05-Mar-2008
Enhancements
	•	The controls area on the right side can now be switched to a name panel. Every signal can be given a name to clarify the usage in a mix setup. The names are shared between all instances and are shown with selectors for the signal color.
	•	The memory switches can now be used in combination with the alt-key to access a complete row with one mouse click, e.g. for storing all signals at the same time.
	•	Pause button added.
	•	Additional zoom buttons for setting the level range.
	•	The maximum peak hold time has been increased from 5 sec to 20 sec.
	•	New measurement tool: By clicking into the frequency display area the mouse cursor changes to a crosshair and shows the frequency and the level at the current position.

Version 2.1.1 - 14-Jan-2008
Enhancements
	•	Instance numbers are now shown in different colors, depending on their state (current, present in setup, unused).

Bug Fixes
	•	FFT mode does now display without requiring audio to be routed through all instances.
	•	Sometimes the plug-in window did not get the focus with the first mouse click (Windows only).

Version 2.1.0 - 14-Sep-2007
Enhancements
	•	New Resolution Option for FFT mode: Full, fractions of octaves (1, 1/2, 1/3, ..., 1/9, 2/3, 3/4).
	•	Manual included.

Bug Fixes
	•	Minor bug fixes.

Version 2.0.0 - 29-Aug-2007
Enhancements
	•	New FFT Mode for the spectrum display: FFT sizes from 512 to 16384 samples, several window options (Rectangular, Hann, Hamming, Blackman, Blackman-Harris, Flat Top), instant display of the FFT result or smooth display according to the Attack and Release settings. Switchable semi-transparent display of the curves for easy detection of overlapping frequency ranges. The 3 selectable display modes (H-Align, V-Align, V-Space) are also usable for the FFT mode whereas the H-Align mode has been renamed to H-Align/Overlay for the overlapping spectrum display. FFT size and window selection are shared across all instances. The visible frequency range can be zoomed with the buttons at the bottom of the spectrum display.
	•	New button Sync Others: Using this button, all other instances can be switched to the same mode (Third Octave or FFT) as the current instance. Useful for reducing the CPU load when many instances are opened.
	•	The Slope knob now has an additional default value of zero. Use left mouse button and shift-control-key (Windows) or shift-command-key (Mac).

Bug Fixes
	•	Negative slope values caused the display of a constant level in third octave mode.
	•	Keyboard focus of the host is now retained after clicking inside the editor window (Mac only).
	•	Compatibility issues with systems running Mac OS X 10.3.

Version 1.2.1 - 11-Jun-2007
Enhancements
	•	The levels of the spectrum display are now scalable in steps of 10 dB with the Plus/Minus buttons on the right.
	•	New display modes added. You can now choose between 3 different display modes by a context menu at the top:
		• H-Align is the already existing mode of the previous versions with horizontally aligned level bars.
		• V-Align adds/aligns the levels vertically without space. This mode provides an instant overview of the frequency distribution of all instances. The height of the level bars is calculated according to the current level range which is shown at the top right of the spectrum display. In this mode the peak settings are without effect and the level grid is numbered only for the first instance. As this mode is intended for relative measurement the level grid always begins with 0 dB at the bottom.
		• V-Space displays the spectrum of every instance in an own view. These views are ordered vertically. 
		The solo/mute switching controls and the memory slots can be applied to all views for selecting the levels to display.
	•	The default color set has been changed for better contrast.
	•	The timeout of the demo version has been increased from 10 to 60 minutes.

Version 1.1.3 - 23-May-2007
Enhancements
	•	Performance improvements.
	•	Switching signals via solo/mute now displays the levels immediately without ramping up according to the Attack setting.

Bug Fixes
	•	Incorrect assignments of levels in low frequency bands if HiRes Mode is deactivated.

Version 1.1.0 - 16-May-2007
Enhancements
	•	New high resolution mode for the low frequency bands. There is a context menu at the top of the GUI to select between the new HiRes Mode and the old Eco Mode. The mode selection is shared across all instances.

Bug Fixes
	•	Incorrect drawing of the GUI after loading a preset under certain circumstances.

Version 1.0.0 - 07-May-2007
	•	Initial Release.